(export (version "E")
  (design
    (source "/tmp/tmp-kibot-net_sch_print-qqupc9nm/Nixie_Tube_Clock.kicad_sch")
    (date "Date")
    (tool "Eeschema 9.0.7+1")
    (textvar (name "ASSEMBLY_NOTES"))
    (textvar (name "BOARD_NAME") "Nixie Clock Main Board")
    (textvar (name "COMPANY") "Company Name")
    (textvar (name "DESIGNER") "Aidan Brzezinski")
    (textvar (name "FABRICATION_NOTES"))
    (textvar (name "GIT_HASH_PCB") "1d094e6")
    (textvar (name "GIT_HASH_SCH") "79f6288")
    (textvar (name "GIT_URL") "https://git.lokislair.com/aidanbrzezinski/Nixie_Tube_Clock.git")
    (textvar (name "PROJECT_NAME") "Nixie Tube Clock")
    (textvar (name "RELEASE_BODY_1.0.0"))
    (textvar (name "RELEASE_BODY_1.0.1"))
    (textvar (name "RELEASE_BODY_1.0.2"))
    (textvar (name "RELEASE_BODY_1.1.0"))
    (textvar (name "RELEASE_BODY_UNRELEASED") "Version Unreleased not found.")
    (textvar (name "RELEASE_DATE") "19-Mar-2026")
    (textvar (name "RELEASE_DATE_NUM") "2026-03-19")
    (textvar (name "RELEASE_TITLE_1.0.0"))
    (textvar (name "RELEASE_TITLE_1.0.1"))
    (textvar (name "RELEASE_TITLE_1.0.2"))
    (textvar (name "RELEASE_TITLE_1.1.0"))
    (textvar (name "RELEASE_TITLE_UNRELEASED") "Version Unreleased not found.")
    (textvar (name "REVISION") "+ (Unreleased)")
    (textvar (name "SHEET_NAME_1") "Cover Page")
    (textvar (name "SHEET_NAME_10") "MUX Inputs - Date Logic")
    (textvar (name "SHEET_NAME_11") "......................................")
    (textvar (name "SHEET_NAME_12") "......................................")
    (textvar (name "SHEET_NAME_13") "......................................")
    (textvar (name "SHEET_NAME_14") "......................................")
    (textvar (name "SHEET_NAME_15") "......................................")
    (textvar (name "SHEET_NAME_16") "......................................")
    (textvar (name "SHEET_NAME_17") "......................................")
    (textvar (name "SHEET_NAME_18") "......................................")
    (textvar (name "SHEET_NAME_19") "......................................")
    (textvar (name "SHEET_NAME_2") "Block Diagram")
    (textvar (name "SHEET_NAME_20") "......................................")
    (textvar (name "SHEET_NAME_21") "......................................")
    (textvar (name "SHEET_NAME_22") "......................................")
    (textvar (name "SHEET_NAME_23") "......................................")
    (textvar (name "SHEET_NAME_24") "......................................")
    (textvar (name "SHEET_NAME_25") "......................................")
    (textvar (name "SHEET_NAME_26") "......................................")
    (textvar (name "SHEET_NAME_27") "......................................")
    (textvar (name "SHEET_NAME_28") "......................................")
    (textvar (name "SHEET_NAME_29") "......................................")
    (textvar (name "SHEET_NAME_3") "Project Architecture")
    (textvar (name "SHEET_NAME_30") "......................................")
    (textvar (name "SHEET_NAME_31") "......................................")
    (textvar (name "SHEET_NAME_32") "......................................")
    (textvar (name "SHEET_NAME_33") "......................................")
    (textvar (name "SHEET_NAME_34") "......................................")
    (textvar (name "SHEET_NAME_35") "......................................")
    (textvar (name "SHEET_NAME_36") "......................................")
    (textvar (name "SHEET_NAME_37") "......................................")
    (textvar (name "SHEET_NAME_38") "......................................")
    (textvar (name "SHEET_NAME_39") "......................................")
    (textvar (name "SHEET_NAME_4") "Clock - Oscillator & Divider")
    (textvar (name "SHEET_NAME_40") "......................................")
    (textvar (name "SHEET_NAME_5") "MUX Inputs - Time Logic")
    (textvar (name "SHEET_NAME_6") "Power - Sequencing")
    (textvar (name "SHEET_NAME_7") "Revision History")
    (textvar (name "SHEET_NAME_8") "MUX Inputs - Anti-Poisoning Logic")
    (textvar (name "SHEET_NAME_9") "Switching MUX")
    (textvar (name "VARIANT") "DRAFT")
    (sheet (number "1") (name "/") (tstamps "/")
      (title_block
        (title)
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "Nixie_Tube_Clock.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "2") (name "/Block Diagram/") (tstamps "/82da9dbf-ba38-4d08-ba35-a220fa2963b1/")
      (title_block
        (title "Block Diagram")
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "Block Diagram.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "3") (name "/Project Architecture/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/")
      (title_block
        (title "Project Architecture")
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "Project Architecture.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "4") (name "/Project Architecture/Clock - Oscillator & Divider/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/f06537ee-772d-44d3-8c50-e0ba41038c9c/")
      (title_block
        (title "Clock")
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "Clock - Oscillator & Divider.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "5") (name "/Project Architecture/MUX Inputs - Time Logic/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/e744f3ce-03a6-44a6-8792-1447ef232b9a/")
      (title_block
        (title "Sheet Title B")
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "Section B - TItle B.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "6") (name "/Power - Sequencing/") (tstamps "/5fb05893-0da3-4f58-a52b-cb6d6f4cb80b/")
      (title_block
        (title "Power - Sequencing")
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "Power - Sequencing.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "7") (name "/Revision History/") (tstamps "/6e125bd6-2f99-4e5d-b3ea-4899f4540739/")
      (title_block
        (title "Revision History")
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "Revision History.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "8") (name "/Project Architecture/MUX Inputs - Anti-Poisoning Logic/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/2a8f5d5f-cd49-42b0-95eb-45963ec7e9fa/")
      (title_block
        (title "Sheet Title B")
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "MUX Inputs - Anti-Poisoning Logic.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "9") (name "/Project Architecture/Switching MUX/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/eafdb10b-8bee-44fc-a926-9f80434f1164/")
      (title_block
        (title "Sheet Title B")
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "Switching MUX.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "10") (name "/Project Architecture/MUX Inputs - Date Logic/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/b0dd3d99-d7aa-4c74-be83-cbd53dc43e16/")
      (title_block
        (title "Sheet Title B")
        (company "Company Name")
        (rev "+ (Unreleased)")
        (date "Date")
        (source "MUX Inputs - Date Logic.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value "")))))
  (components
    (comp (ref "U1")
      (value "4020")
      (datasheet "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4020bms-24bms-40bms.pdf")
      (description "Binary counter 14 stages (asynchronous)")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4020bms-24bms-40bms.pdf")
        (field (name "Description") "Binary counter 14 stages (asynchronous)"))
      (libsource (lib "4xxx") (part "4020") (description "Binary counter 14 stages (asynchronous)"))
      (property (name "Sheetname") (value "Clock - Oscillator & Divider"))
      (property (name "Sheetfile") (value "Clock - Oscillator & Divider.kicad_sch"))
      (property (name "ki_keywords") (value "CMOS CNT CNT14"))
      (property (name "ki_fp_filters") (value "DIP?16*"))
      (sheetpath (names "/Project Architecture/Clock - Oscillator & Divider/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/f06537ee-772d-44d3-8c50-e0ba41038c9c/"))
      (tstamps "48110268-f09a-460b-98ce-8d80141bae2f"))
    (comp (ref "U2")
      (value "4060")
      (datasheet "https://www.st.com/resource/en/datasheet/m74hc4060.pdf")
      (description "Binary counter (14-stages) and oscillator")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "https://www.st.com/resource/en/datasheet/m74hc4060.pdf")
        (field (name "Description") "Binary counter (14-stages) and oscillator"))
      (libsource (lib "4xxx") (part "4060") (description "Binary counter (14-stages) and oscillator"))
      (property (name "Sheetname") (value "Clock - Oscillator & Divider"))
      (property (name "Sheetfile") (value "Clock - Oscillator & Divider.kicad_sch"))
      (property (name "ki_keywords") (value "binary counter oscillator"))
      (property (name "ki_fp_filters") (value "DIP?16*7.62* TSSOP*16*4.4x5* SOIC*16*3.9x9.9*"))
      (sheetpath (names "/Project Architecture/Clock - Oscillator & Divider/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/f06537ee-772d-44d3-8c50-e0ba41038c9c/"))
      (tstamps "ad915d92-65e5-4de4-b04e-3a55aecd6da3"))
    (comp (ref "U3")
      (value "74HC193")
      (datasheet "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
      (description "Synchronous 4-bit Up/Down (2 clk) counter")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
        (field (name "Description") "Synchronous 4-bit Up/Down (2 clk) counter"))
      (libsource (lib "74xx") (part "74HC193") (description "Synchronous 4-bit Up/Down (2 clk) counter"))
      (property (name "Sheetname") (value "MUX Inputs - Time Logic"))
      (property (name "Sheetfile") (value "Section B - TItle B.kicad_sch"))
      (property (name "ki_keywords") (value "TTL CNT CNT4"))
      (property (name "ki_fp_filters") (value "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm* SO*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"))
      (sheetpath (names "/Project Architecture/MUX Inputs - Time Logic/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/e744f3ce-03a6-44a6-8792-1447ef232b9a/"))
      (tstamps "81b3c978-4984-4503-a138-a2856bde09b4"))
    (comp (ref "U4")
      (value "74HC193")
      (datasheet "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
      (description "Synchronous 4-bit Up/Down (2 clk) counter")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
        (field (name "Description") "Synchronous 4-bit Up/Down (2 clk) counter"))
      (libsource (lib "74xx") (part "74HC193") (description "Synchronous 4-bit Up/Down (2 clk) counter"))
      (property (name "Sheetname") (value "MUX Inputs - Time Logic"))
      (property (name "Sheetfile") (value "Section B - TItle B.kicad_sch"))
      (property (name "ki_keywords") (value "TTL CNT CNT4"))
      (property (name "ki_fp_filters") (value "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm* SO*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"))
      (sheetpath (names "/Project Architecture/MUX Inputs - Time Logic/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/e744f3ce-03a6-44a6-8792-1447ef232b9a/"))
      (tstamps "9b17f9b0-0d1e-4936-a3d7-dfd853821123"))
    (comp (ref "U5")
      (value "74HC193")
      (datasheet "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
      (description "Synchronous 4-bit Up/Down (2 clk) counter")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
        (field (name "Description") "Synchronous 4-bit Up/Down (2 clk) counter"))
      (libsource (lib "74xx") (part "74HC193") (description "Synchronous 4-bit Up/Down (2 clk) counter"))
      (property (name "Sheetname") (value "MUX Inputs - Time Logic"))
      (property (name "Sheetfile") (value "Section B - TItle B.kicad_sch"))
      (property (name "ki_keywords") (value "TTL CNT CNT4"))
      (property (name "ki_fp_filters") (value "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm* SO*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"))
      (sheetpath (names "/Project Architecture/MUX Inputs - Time Logic/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/e744f3ce-03a6-44a6-8792-1447ef232b9a/"))
      (tstamps "c8a10d89-61aa-4d03-9fb5-f91b06c26e91"))
    (comp (ref "U6")
      (value "74HC193")
      (datasheet "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
      (description "Synchronous 4-bit Up/Down (2 clk) counter")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
        (field (name "Description") "Synchronous 4-bit Up/Down (2 clk) counter"))
      (libsource (lib "74xx") (part "74HC193") (description "Synchronous 4-bit Up/Down (2 clk) counter"))
      (property (name "Sheetname") (value "MUX Inputs - Time Logic"))
      (property (name "Sheetfile") (value "Section B - TItle B.kicad_sch"))
      (property (name "ki_keywords") (value "TTL CNT CNT4"))
      (property (name "ki_fp_filters") (value "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm* SO*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"))
      (sheetpath (names "/Project Architecture/MUX Inputs - Time Logic/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/e744f3ce-03a6-44a6-8792-1447ef232b9a/"))
      (tstamps "a51c4a69-025b-430e-8dd0-7a08217094f9"))
    (comp (ref "U7")
      (value "74HC193")
      (datasheet "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
      (description "Synchronous 4-bit Up/Down (2 clk) counter")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
        (field (name "Description") "Synchronous 4-bit Up/Down (2 clk) counter"))
      (libsource (lib "74xx") (part "74HC193") (description "Synchronous 4-bit Up/Down (2 clk) counter"))
      (property (name "Sheetname") (value "MUX Inputs - Time Logic"))
      (property (name "Sheetfile") (value "Section B - TItle B.kicad_sch"))
      (property (name "ki_keywords") (value "TTL CNT CNT4"))
      (property (name "ki_fp_filters") (value "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm* SO*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"))
      (sheetpath (names "/Project Architecture/MUX Inputs - Time Logic/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/e744f3ce-03a6-44a6-8792-1447ef232b9a/"))
      (tstamps "303ecea9-1618-41c7-b515-b253b054f479"))
    (comp (ref "U8")
      (value "74HC193")
      (datasheet "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
      (description "Synchronous 4-bit Up/Down (2 clk) counter")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
        (field (name "Description") "Synchronous 4-bit Up/Down (2 clk) counter"))
      (libsource (lib "74xx") (part "74HC193") (description "Synchronous 4-bit Up/Down (2 clk) counter"))
      (property (name "Sheetname") (value "MUX Inputs - Time Logic"))
      (property (name "Sheetfile") (value "Section B - TItle B.kicad_sch"))
      (property (name "ki_keywords") (value "TTL CNT CNT4"))
      (property (name "ki_fp_filters") (value "SOIC*3.9x9.9mm*P1.27mm* DIP*W7.62mm* SO*3.9*9.9mm*P1.27mm* TSSOP*4.4*5mm*P0.65mm*"))
      (sheetpath (names "/Project Architecture/MUX Inputs - Time Logic/") (tstamps "/c5103ceb-5325-4a84-a025-9638a412984e/e744f3ce-03a6-44a6-8792-1447ef232b9a/"))
      (tstamps "e5cc581d-b6c6-4efe-9a32-40abab369b78")))
  (libparts
    (libpart (lib "4xxx") (part "4020")
      (description "Binary counter 14 stages (asynchronous)")
      (docs "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4020bms-24bms-40bms.pdf")
      (footprints
        (fp "DIP?16*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "4020")
        (field (name "Footprint"))
        (field (name "Datasheet") "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4020bms-24bms-40bms.pdf")
        (field (name "Description") "Binary counter 14 stages (asynchronous)"))
      (pins
        (pin (num "1") (name "Q11") (type "output"))
        (pin (num "2") (name "Q12") (type "output"))
        (pin (num "3") (name "Q13") (type "output"))
        (pin (num "4") (name "Q5") (type "output"))
        (pin (num "5") (name "Q4") (type "output"))
        (pin (num "6") (name "Q6") (type "output"))
        (pin (num "7") (name "Q3") (type "output"))
        (pin (num "8") (name "VSS") (type "power_in"))
        (pin (num "9") (name "Q0") (type "output"))
        (pin (num "10") (name "CLK") (type "input"))
        (pin (num "11") (name "Reset") (type "input"))
        (pin (num "12") (name "Q8") (type "output"))
        (pin (num "13") (name "Q7") (type "output"))
        (pin (num "14") (name "Q9") (type "output"))
        (pin (num "15") (name "Q10") (type "output"))
        (pin (num "16") (name "VDD") (type "power_in"))))
    (libpart (lib "4xxx") (part "4060")
      (description "Binary counter (14-stages) and oscillator")
      (docs "https://www.st.com/resource/en/datasheet/m74hc4060.pdf")
      (footprints
        (fp "DIP?16*7.62*")
        (fp "TSSOP*16*4.4x5*")
        (fp "SOIC*16*3.9x9.9*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "4060")
        (field (name "Footprint"))
        (field (name "Datasheet") "https://www.st.com/resource/en/datasheet/m74hc4060.pdf")
        (field (name "Description") "Binary counter (14-stages) and oscillator"))
      (pins
        (pin (num "1") (name "Q12") (type "output"))
        (pin (num "2") (name "Q13") (type "output"))
        (pin (num "3") (name "Q14") (type "output"))
        (pin (num "4") (name "Q6") (type "output"))
        (pin (num "5") (name "Q5") (type "output"))
        (pin (num "6") (name "Q7") (type "output"))
        (pin (num "7") (name "Q4") (type "output"))
        (pin (num "8") (name "VSS") (type "power_in"))
        (pin (num "9") (name "~{Φ0}") (type "input"))
        (pin (num "10") (name "Φ0") (type "input"))
        (pin (num "11") (name "~{Φ1}") (type "input"))
        (pin (num "12") (name "CLR") (type "input"))
        (pin (num "13") (name "Q9") (type "output"))
        (pin (num "14") (name "Q8") (type "output"))
        (pin (num "15") (name "Q10") (type "output"))
        (pin (num "16") (name "VDD") (type "power_in"))))
    (libpart (lib "74xx") (part "74HC193")
      (description "Synchronous 4-bit Up/Down (2 clk) counter")
      (docs "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
      (footprints
        (fp "SOIC*3.9x9.9mm*P1.27mm*")
        (fp "DIP*W7.62mm*")
        (fp "SO*3.9*9.9mm*P1.27mm*")
        (fp "TSSOP*4.4*5mm*P0.65mm*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "74HC193")
        (field (name "Footprint"))
        (field (name "Datasheet") "https://assets.nexperia.com/documents/data-sheet/74HC_HCT193.pdf")
        (field (name "Description") "Synchronous 4-bit Up/Down (2 clk) counter"))
      (pins
        (pin (num "1") (name "B") (type "input"))
        (pin (num "2") (name "QB") (type "output"))
        (pin (num "3") (name "QA") (type "output"))
        (pin (num "4") (name "DOWN") (type "input"))
        (pin (num "5") (name "UP") (type "input"))
        (pin (num "6") (name "QC") (type "output"))
        (pin (num "7") (name "QD") (type "output"))
        (pin (num "8") (name "GND") (type "power_in"))
        (pin (num "9") (name "D") (type "input"))
        (pin (num "10") (name "C") (type "input"))
        (pin (num "11") (name "~{LOAD}") (type "input"))
        (pin (num "12") (name "~{CO}") (type "output"))
        (pin (num "13") (name "~{BO}") (type "output"))
        (pin (num "14") (name "CLR") (type "input"))
        (pin (num "15") (name "A") (type "input"))
        (pin (num "16") (name "VCC") (type "power_in")))))
  (libraries
    (library (logical "4xxx")
      (uri "/usr/share/kicad/symbols/4xxx.kicad_sym"))
    (library (logical "74xx")
      (uri "/usr/share/kicad/symbols/74xx.kicad_sym")))
  (nets
    (net (code "1") (name "unconnected-(U1-CLK-Pad10)") (class "Default")
      (node (ref "U1") (pin "10") (pinfunction "CLK") (pintype "input")))
    (net (code "2") (name "unconnected-(U1-Q0-Pad9)") (class "Default")
      (node (ref "U1") (pin "9") (pinfunction "Q0") (pintype "output")))
    (net (code "3") (name "unconnected-(U1-Q3-Pad7)") (class "Default")
      (node (ref "U1") (pin "7") (pinfunction "Q3") (pintype "output")))
    (net (code "4") (name "unconnected-(U1-Q4-Pad5)") (class "Default")
      (node (ref "U1") (pin "5") (pinfunction "Q4") (pintype "output")))
    (net (code "5") (name "unconnected-(U1-Q5-Pad4)") (class "Default")
      (node (ref "U1") (pin "4") (pinfunction "Q5") (pintype "output")))
    (net (code "6") (name "unconnected-(U1-Q6-Pad6)") (class "Default")
      (node (ref "U1") (pin "6") (pinfunction "Q6") (pintype "output")))
    (net (code "7") (name "unconnected-(U1-Q7-Pad13)") (class "Default")
      (node (ref "U1") (pin "13") (pinfunction "Q7") (pintype "output")))
    (net (code "8") (name "unconnected-(U1-Q8-Pad12)") (class "Default")
      (node (ref "U1") (pin "12") (pinfunction "Q8") (pintype "output")))
    (net (code "9") (name "unconnected-(U1-Q9-Pad14)") (class "Default")
      (node (ref "U1") (pin "14") (pinfunction "Q9") (pintype "output")))
    (net (code "10") (name "unconnected-(U1-Q10-Pad15)") (class "Default")
      (node (ref "U1") (pin "15") (pinfunction "Q10") (pintype "output")))
    (net (code "11") (name "unconnected-(U1-Q11-Pad1)") (class "Default")
      (node (ref "U1") (pin "1") (pinfunction "Q11") (pintype "output")))
    (net (code "12") (name "unconnected-(U1-Q12-Pad2)") (class "Default")
      (node (ref "U1") (pin "2") (pinfunction "Q12") (pintype "output")))
    (net (code "13") (name "unconnected-(U1-Q13-Pad3)") (class "Default")
      (node (ref "U1") (pin "3") (pinfunction "Q13") (pintype "output")))
    (net (code "14") (name "unconnected-(U1-Reset-Pad11)") (class "Default")
      (node (ref "U1") (pin "11") (pinfunction "Reset") (pintype "input")))
    (net (code "15") (name "unconnected-(U1-VDD-Pad16)") (class "Default")
      (node (ref "U1") (pin "16") (pinfunction "VDD") (pintype "power_in")))
    (net (code "16") (name "unconnected-(U1-VSS-Pad8)") (class "Default")
      (node (ref "U1") (pin "8") (pinfunction "VSS") (pintype "power_in")))
    (net (code "17") (name "unconnected-(U2-CLR-Pad12)") (class "Default")
      (node (ref "U2") (pin "12") (pinfunction "CLR") (pintype "input")))
    (net (code "18") (name "unconnected-(U2-Q4-Pad7)") (class "Default")
      (node (ref "U2") (pin "7") (pinfunction "Q4") (pintype "output")))
    (net (code "19") (name "unconnected-(U2-Q5-Pad5)") (class "Default")
      (node (ref "U2") (pin "5") (pinfunction "Q5") (pintype "output")))
    (net (code "20") (name "unconnected-(U2-Q6-Pad4)") (class "Default")
      (node (ref "U2") (pin "4") (pinfunction "Q6") (pintype "output")))
    (net (code "21") (name "unconnected-(U2-Q7-Pad6)") (class "Default")
      (node (ref "U2") (pin "6") (pinfunction "Q7") (pintype "output")))
    (net (code "22") (name "unconnected-(U2-Q8-Pad14)") (class "Default")
      (node (ref "U2") (pin "14") (pinfunction "Q8") (pintype "output")))
    (net (code "23") (name "unconnected-(U2-Q9-Pad13)") (class "Default")
      (node (ref "U2") (pin "13") (pinfunction "Q9") (pintype "output")))
    (net (code "24") (name "unconnected-(U2-Q10-Pad15)") (class "Default")
      (node (ref "U2") (pin "15") (pinfunction "Q10") (pintype "output")))
    (net (code "25") (name "unconnected-(U2-Q12-Pad1)") (class "Default")
      (node (ref "U2") (pin "1") (pinfunction "Q12") (pintype "output")))
    (net (code "26") (name "unconnected-(U2-Q13-Pad2)") (class "Default")
      (node (ref "U2") (pin "2") (pinfunction "Q13") (pintype "output")))
    (net (code "27") (name "unconnected-(U2-Q14-Pad3)") (class "Default")
      (node (ref "U2") (pin "3") (pinfunction "Q14") (pintype "output")))
    (net (code "28") (name "unconnected-(U2-VDD-Pad16)") (class "Default")
      (node (ref "U2") (pin "16") (pinfunction "VDD") (pintype "power_in")))
    (net (code "29") (name "unconnected-(U2-VSS-Pad8)") (class "Default")
      (node (ref "U2") (pin "8") (pinfunction "VSS") (pintype "power_in")))
    (net (code "30") (name "unconnected-(U2-~{Φ0}-Pad9)") (class "Default")
      (node (ref "U2") (pin "9") (pinfunction "~{Φ0}") (pintype "input")))
    (net (code "31") (name "unconnected-(U2-~{Φ1}-Pad11)") (class "Default")
      (node (ref "U2") (pin "11") (pinfunction "~{Φ1}") (pintype "input")))
    (net (code "32") (name "unconnected-(U2-Φ0-Pad10)") (class "Default")
      (node (ref "U2") (pin "10") (pinfunction "Φ0") (pintype "input")))
    (net (code "33") (name "unconnected-(U3-A-Pad15)") (class "Default")
      (node (ref "U3") (pin "15") (pinfunction "A") (pintype "input")))
    (net (code "34") (name "unconnected-(U3-B-Pad1)") (class "Default")
      (node (ref "U3") (pin "1") (pinfunction "B") (pintype "input")))
    (net (code "35") (name "unconnected-(U3-C-Pad10)") (class "Default")
      (node (ref "U3") (pin "10") (pinfunction "C") (pintype "input")))
    (net (code "36") (name "unconnected-(U3-CLR-Pad14)") (class "Default")
      (node (ref "U3") (pin "14") (pinfunction "CLR") (pintype "input")))
    (net (code "37") (name "unconnected-(U3-D-Pad9)") (class "Default")
      (node (ref "U3") (pin "9") (pinfunction "D") (pintype "input")))
    (net (code "38") (name "unconnected-(U3-DOWN-Pad4)") (class "Default")
      (node (ref "U3") (pin "4") (pinfunction "DOWN") (pintype "input")))
    (net (code "39") (name "unconnected-(U3-GND-Pad8)") (class "Default")
      (node (ref "U3") (pin "8") (pinfunction "GND") (pintype "power_in")))
    (net (code "40") (name "unconnected-(U3-QA-Pad3)") (class "Default")
      (node (ref "U3") (pin "3") (pinfunction "QA") (pintype "output")))
    (net (code "41") (name "unconnected-(U3-QB-Pad2)") (class "Default")
      (node (ref "U3") (pin "2") (pinfunction "QB") (pintype "output")))
    (net (code "42") (name "unconnected-(U3-QC-Pad6)") (class "Default")
      (node (ref "U3") (pin "6") (pinfunction "QC") (pintype "output")))
    (net (code "43") (name "unconnected-(U3-QD-Pad7)") (class "Default")
      (node (ref "U3") (pin "7") (pinfunction "QD") (pintype "output")))
    (net (code "44") (name "unconnected-(U3-UP-Pad5)") (class "Default")
      (node (ref "U3") (pin "5") (pinfunction "UP") (pintype "input")))
    (net (code "45") (name "unconnected-(U3-VCC-Pad16)") (class "Default")
      (node (ref "U3") (pin "16") (pinfunction "VCC") (pintype "power_in")))
    (net (code "46") (name "unconnected-(U3-~{BO}-Pad13)") (class "Default")
      (node (ref "U3") (pin "13") (pinfunction "~{BO}") (pintype "output")))
    (net (code "47") (name "unconnected-(U3-~{CO}-Pad12)") (class "Default")
      (node (ref "U3") (pin "12") (pinfunction "~{CO}") (pintype "output")))
    (net (code "48") (name "unconnected-(U3-~{LOAD}-Pad11)") (class "Default")
      (node (ref "U3") (pin "11") (pinfunction "~{LOAD}") (pintype "input")))
    (net (code "49") (name "unconnected-(U4-A-Pad15)") (class "Default")
      (node (ref "U4") (pin "15") (pinfunction "A") (pintype "input")))
    (net (code "50") (name "unconnected-(U4-B-Pad1)") (class "Default")
      (node (ref "U4") (pin "1") (pinfunction "B") (pintype "input")))
    (net (code "51") (name "unconnected-(U4-C-Pad10)") (class "Default")
      (node (ref "U4") (pin "10") (pinfunction "C") (pintype "input")))
    (net (code "52") (name "unconnected-(U4-CLR-Pad14)") (class "Default")
      (node (ref "U4") (pin "14") (pinfunction "CLR") (pintype "input")))
    (net (code "53") (name "unconnected-(U4-D-Pad9)") (class "Default")
      (node (ref "U4") (pin "9") (pinfunction "D") (pintype "input")))
    (net (code "54") (name "unconnected-(U4-DOWN-Pad4)") (class "Default")
      (node (ref "U4") (pin "4") (pinfunction "DOWN") (pintype "input")))
    (net (code "55") (name "unconnected-(U4-GND-Pad8)") (class "Default")
      (node (ref "U4") (pin "8") (pinfunction "GND") (pintype "power_in")))
    (net (code "56") (name "unconnected-(U4-QA-Pad3)") (class "Default")
      (node (ref "U4") (pin "3") (pinfunction "QA") (pintype "output")))
    (net (code "57") (name "unconnected-(U4-QB-Pad2)") (class "Default")
      (node (ref "U4") (pin "2") (pinfunction "QB") (pintype "output")))
    (net (code "58") (name "unconnected-(U4-QC-Pad6)") (class "Default")
      (node (ref "U4") (pin "6") (pinfunction "QC") (pintype "output")))
    (net (code "59") (name "unconnected-(U4-QD-Pad7)") (class "Default")
      (node (ref "U4") (pin "7") (pinfunction "QD") (pintype "output")))
    (net (code "60") (name "unconnected-(U4-UP-Pad5)") (class "Default")
      (node (ref "U4") (pin "5") (pinfunction "UP") (pintype "input")))
    (net (code "61") (name "unconnected-(U4-VCC-Pad16)") (class "Default")
      (node (ref "U4") (pin "16") (pinfunction "VCC") (pintype "power_in")))
    (net (code "62") (name "unconnected-(U4-~{BO}-Pad13)") (class "Default")
      (node (ref "U4") (pin "13") (pinfunction "~{BO}") (pintype "output")))
    (net (code "63") (name "unconnected-(U4-~{CO}-Pad12)") (class "Default")
      (node (ref "U4") (pin "12") (pinfunction "~{CO}") (pintype "output")))
    (net (code "64") (name "unconnected-(U4-~{LOAD}-Pad11)") (class "Default")
      (node (ref "U4") (pin "11") (pinfunction "~{LOAD}") (pintype "input")))
    (net (code "65") (name "unconnected-(U5-A-Pad15)") (class "Default")
      (node (ref "U5") (pin "15") (pinfunction "A") (pintype "input")))
    (net (code "66") (name "unconnected-(U5-B-Pad1)") (class "Default")
      (node (ref "U5") (pin "1") (pinfunction "B") (pintype "input")))
    (net (code "67") (name "unconnected-(U5-C-Pad10)") (class "Default")
      (node (ref "U5") (pin "10") (pinfunction "C") (pintype "input")))
    (net (code "68") (name "unconnected-(U5-CLR-Pad14)") (class "Default")
      (node (ref "U5") (pin "14") (pinfunction "CLR") (pintype "input")))
    (net (code "69") (name "unconnected-(U5-D-Pad9)") (class "Default")
      (node (ref "U5") (pin "9") (pinfunction "D") (pintype "input")))
    (net (code "70") (name "unconnected-(U5-DOWN-Pad4)") (class "Default")
      (node (ref "U5") (pin "4") (pinfunction "DOWN") (pintype "input")))
    (net (code "71") (name "unconnected-(U5-GND-Pad8)") (class "Default")
      (node (ref "U5") (pin "8") (pinfunction "GND") (pintype "power_in")))
    (net (code "72") (name "unconnected-(U5-QA-Pad3)") (class "Default")
      (node (ref "U5") (pin "3") (pinfunction "QA") (pintype "output")))
    (net (code "73") (name "unconnected-(U5-QB-Pad2)") (class "Default")
      (node (ref "U5") (pin "2") (pinfunction "QB") (pintype "output")))
    (net (code "74") (name "unconnected-(U5-QC-Pad6)") (class "Default")
      (node (ref "U5") (pin "6") (pinfunction "QC") (pintype "output")))
    (net (code "75") (name "unconnected-(U5-QD-Pad7)") (class "Default")
      (node (ref "U5") (pin "7") (pinfunction "QD") (pintype "output")))
    (net (code "76") (name "unconnected-(U5-UP-Pad5)") (class "Default")
      (node (ref "U5") (pin "5") (pinfunction "UP") (pintype "input")))
    (net (code "77") (name "unconnected-(U5-VCC-Pad16)") (class "Default")
      (node (ref "U5") (pin "16") (pinfunction "VCC") (pintype "power_in")))
    (net (code "78") (name "unconnected-(U5-~{BO}-Pad13)") (class "Default")
      (node (ref "U5") (pin "13") (pinfunction "~{BO}") (pintype "output")))
    (net (code "79") (name "unconnected-(U5-~{CO}-Pad12)") (class "Default")
      (node (ref "U5") (pin "12") (pinfunction "~{CO}") (pintype "output")))
    (net (code "80") (name "unconnected-(U5-~{LOAD}-Pad11)") (class "Default")
      (node (ref "U5") (pin "11") (pinfunction "~{LOAD}") (pintype "input")))
    (net (code "81") (name "unconnected-(U6-A-Pad15)") (class "Default")
      (node (ref "U6") (pin "15") (pinfunction "A") (pintype "input")))
    (net (code "82") (name "unconnected-(U6-B-Pad1)") (class "Default")
      (node (ref "U6") (pin "1") (pinfunction "B") (pintype "input")))
    (net (code "83") (name "unconnected-(U6-C-Pad10)") (class "Default")
      (node (ref "U6") (pin "10") (pinfunction "C") (pintype "input")))
    (net (code "84") (name "unconnected-(U6-CLR-Pad14)") (class "Default")
      (node (ref "U6") (pin "14") (pinfunction "CLR") (pintype "input")))
    (net (code "85") (name "unconnected-(U6-D-Pad9)") (class "Default")
      (node (ref "U6") (pin "9") (pinfunction "D") (pintype "input")))
    (net (code "86") (name "unconnected-(U6-DOWN-Pad4)") (class "Default")
      (node (ref "U6") (pin "4") (pinfunction "DOWN") (pintype "input")))
    (net (code "87") (name "unconnected-(U6-GND-Pad8)") (class "Default")
      (node (ref "U6") (pin "8") (pinfunction "GND") (pintype "power_in")))
    (net (code "88") (name "unconnected-(U6-QA-Pad3)") (class "Default")
      (node (ref "U6") (pin "3") (pinfunction "QA") (pintype "output")))
    (net (code "89") (name "unconnected-(U6-QB-Pad2)") (class "Default")
      (node (ref "U6") (pin "2") (pinfunction "QB") (pintype "output")))
    (net (code "90") (name "unconnected-(U6-QC-Pad6)") (class "Default")
      (node (ref "U6") (pin "6") (pinfunction "QC") (pintype "output")))
    (net (code "91") (name "unconnected-(U6-QD-Pad7)") (class "Default")
      (node (ref "U6") (pin "7") (pinfunction "QD") (pintype "output")))
    (net (code "92") (name "unconnected-(U6-UP-Pad5)") (class "Default")
      (node (ref "U6") (pin "5") (pinfunction "UP") (pintype "input")))
    (net (code "93") (name "unconnected-(U6-VCC-Pad16)") (class "Default")
      (node (ref "U6") (pin "16") (pinfunction "VCC") (pintype "power_in")))
    (net (code "94") (name "unconnected-(U6-~{BO}-Pad13)") (class "Default")
      (node (ref "U6") (pin "13") (pinfunction "~{BO}") (pintype "output")))
    (net (code "95") (name "unconnected-(U6-~{CO}-Pad12)") (class "Default")
      (node (ref "U6") (pin "12") (pinfunction "~{CO}") (pintype "output")))
    (net (code "96") (name "unconnected-(U6-~{LOAD}-Pad11)") (class "Default")
      (node (ref "U6") (pin "11") (pinfunction "~{LOAD}") (pintype "input")))
    (net (code "97") (name "unconnected-(U7-A-Pad15)") (class "Default")
      (node (ref "U7") (pin "15") (pinfunction "A") (pintype "input")))
    (net (code "98") (name "unconnected-(U7-B-Pad1)") (class "Default")
      (node (ref "U7") (pin "1") (pinfunction "B") (pintype "input")))
    (net (code "99") (name "unconnected-(U7-C-Pad10)") (class "Default")
      (node (ref "U7") (pin "10") (pinfunction "C") (pintype "input")))
    (net (code "100") (name "unconnected-(U7-CLR-Pad14)") (class "Default")
      (node (ref "U7") (pin "14") (pinfunction "CLR") (pintype "input")))
    (net (code "101") (name "unconnected-(U7-D-Pad9)") (class "Default")
      (node (ref "U7") (pin "9") (pinfunction "D") (pintype "input")))
    (net (code "102") (name "unconnected-(U7-DOWN-Pad4)") (class "Default")
      (node (ref "U7") (pin "4") (pinfunction "DOWN") (pintype "input")))
    (net (code "103") (name "unconnected-(U7-GND-Pad8)") (class "Default")
      (node (ref "U7") (pin "8") (pinfunction "GND") (pintype "power_in")))
    (net (code "104") (name "unconnected-(U7-QA-Pad3)") (class "Default")
      (node (ref "U7") (pin "3") (pinfunction "QA") (pintype "output")))
    (net (code "105") (name "unconnected-(U7-QB-Pad2)") (class "Default")
      (node (ref "U7") (pin "2") (pinfunction "QB") (pintype "output")))
    (net (code "106") (name "unconnected-(U7-QC-Pad6)") (class "Default")
      (node (ref "U7") (pin "6") (pinfunction "QC") (pintype "output")))
    (net (code "107") (name "unconnected-(U7-QD-Pad7)") (class "Default")
      (node (ref "U7") (pin "7") (pinfunction "QD") (pintype "output")))
    (net (code "108") (name "unconnected-(U7-UP-Pad5)") (class "Default")
      (node (ref "U7") (pin "5") (pinfunction "UP") (pintype "input")))
    (net (code "109") (name "unconnected-(U7-VCC-Pad16)") (class "Default")
      (node (ref "U7") (pin "16") (pinfunction "VCC") (pintype "power_in")))
    (net (code "110") (name "unconnected-(U7-~{BO}-Pad13)") (class "Default")
      (node (ref "U7") (pin "13") (pinfunction "~{BO}") (pintype "output")))
    (net (code "111") (name "unconnected-(U7-~{CO}-Pad12)") (class "Default")
      (node (ref "U7") (pin "12") (pinfunction "~{CO}") (pintype "output")))
    (net (code "112") (name "unconnected-(U7-~{LOAD}-Pad11)") (class "Default")
      (node (ref "U7") (pin "11") (pinfunction "~{LOAD}") (pintype "input")))
    (net (code "113") (name "unconnected-(U8-A-Pad15)") (class "Default")
      (node (ref "U8") (pin "15") (pinfunction "A") (pintype "input")))
    (net (code "114") (name "unconnected-(U8-B-Pad1)") (class "Default")
      (node (ref "U8") (pin "1") (pinfunction "B") (pintype "input")))
    (net (code "115") (name "unconnected-(U8-C-Pad10)") (class "Default")
      (node (ref "U8") (pin "10") (pinfunction "C") (pintype "input")))
    (net (code "116") (name "unconnected-(U8-CLR-Pad14)") (class "Default")
      (node (ref "U8") (pin "14") (pinfunction "CLR") (pintype "input")))
    (net (code "117") (name "unconnected-(U8-D-Pad9)") (class "Default")
      (node (ref "U8") (pin "9") (pinfunction "D") (pintype "input")))
    (net (code "118") (name "unconnected-(U8-DOWN-Pad4)") (class "Default")
      (node (ref "U8") (pin "4") (pinfunction "DOWN") (pintype "input")))
    (net (code "119") (name "unconnected-(U8-GND-Pad8)") (class "Default")
      (node (ref "U8") (pin "8") (pinfunction "GND") (pintype "power_in")))
    (net (code "120") (name "unconnected-(U8-QA-Pad3)") (class "Default")
      (node (ref "U8") (pin "3") (pinfunction "QA") (pintype "output")))
    (net (code "121") (name "unconnected-(U8-QB-Pad2)") (class "Default")
      (node (ref "U8") (pin "2") (pinfunction "QB") (pintype "output")))
    (net (code "122") (name "unconnected-(U8-QC-Pad6)") (class "Default")
      (node (ref "U8") (pin "6") (pinfunction "QC") (pintype "output")))
    (net (code "123") (name "unconnected-(U8-QD-Pad7)") (class "Default")
      (node (ref "U8") (pin "7") (pinfunction "QD") (pintype "output")))
    (net (code "124") (name "unconnected-(U8-UP-Pad5)") (class "Default")
      (node (ref "U8") (pin "5") (pinfunction "UP") (pintype "input")))
    (net (code "125") (name "unconnected-(U8-VCC-Pad16)") (class "Default")
      (node (ref "U8") (pin "16") (pinfunction "VCC") (pintype "power_in")))
    (net (code "126") (name "unconnected-(U8-~{BO}-Pad13)") (class "Default")
      (node (ref "U8") (pin "13") (pinfunction "~{BO}") (pintype "output")))
    (net (code "127") (name "unconnected-(U8-~{CO}-Pad12)") (class "Default")
      (node (ref "U8") (pin "12") (pinfunction "~{CO}") (pintype "output")))
    (net (code "128") (name "unconnected-(U8-~{LOAD}-Pad11)") (class "Default")
      (node (ref "U8") (pin "11") (pinfunction "~{LOAD}") (pintype "input")))))