(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(uuid "ea8c4f5e-7a49-4faf-a994-dbc85ed86b0a")
	(paper "A4")
	(title_block
		(title "Clock")
		(date "2025-01-12")
		(rev "${REVISION}")
		(company "${COMPANY}")
	)
	(lib_symbols
		(symbol "4xxx:4020"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -7.62 16.51 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "4020"
				(at -7.62 -19.05 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4020bms-24bms-40bms.pdf"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Binary counter 14 stages (asynchronous)"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "ki_keywords" "CMOS CNT CNT14"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "DIP?16*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "4020_1_0"
				(pin input inverted_clock
					(at -12.7 12.7 0)
					(length 5.08)
					(name "CLK"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "10"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -12.7 7.62 0)
					(length 5.08)
					(name "Reset"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "11"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 20.32 270)
					(length 5.08)
					(name "VDD"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "16"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 -22.86 90)
					(length 5.08)
					(name "VSS"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "8"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 12.7 180)
					(length 5.08)
					(name "Q0"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "9"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 10.16 180)
					(length 5.08)
					(name "Q3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "7"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 7.62 180)
					(length 5.08)
					(name "Q4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 5.08 180)
					(length 5.08)
					(name "Q5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 2.54 180)
					(length 5.08)
					(name "Q6"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "6"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 0 180)
					(length 5.08)
					(name "Q7"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "13"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -2.54 180)
					(length 5.08)
					(name "Q8"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "12"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -5.08 180)
					(length 5.08)
					(name "Q9"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "14"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -7.62 180)
					(length 5.08)
					(name "Q10"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "15"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -10.16 180)
					(length 5.08)
					(name "Q11"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -12.7 180)
					(length 5.08)
					(name "Q12"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -15.24 180)
					(length 5.08)
					(name "Q13"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(symbol "4020_1_1"
				(rectangle
					(start -7.62 15.24)
					(end 7.62 -17.78)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "4xxx:4060"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 5.08 16.51 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "4060"
				(at 6.35 -16.51 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 -2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/m74hc4060.pdf"
				(at 0 -5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Binary counter (14-stages) and oscillator"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "binary counter oscillator"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "DIP?16*7.62* TSSOP*16*4.4x5* SOIC*16*3.9x9.9*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "4060_1_0"
				(pin input inverted_clock
					(at -12.7 12.7 0)
					(length 5.08)
					(name "~{Φ0}"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "9"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input clock
					(at -12.7 10.16 0)
					(length 5.08)
					(name "Φ0"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "10"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input inverted_clock
					(at -12.7 7.62 0)
					(length 5.08)
					(name "~{Φ1}"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "11"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -12.7 2.54 0)
					(length 5.08)
					(name "CLR"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "12"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 20.32 270)
					(length 5.08)
					(name "VDD"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "16"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 -20.32 90)
					(length 5.08)
					(name "VSS"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "8"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 12.7 180)
					(length 5.08)
					(name "Q4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "7"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 10.16 180)
					(length 5.08)
					(name "Q5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 7.62 180)
					(length 5.08)
					(name "Q6"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 5.08 180)
					(length 5.08)
					(name "Q7"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "6"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 2.54 180)
					(length 5.08)
					(name "Q8"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "14"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 0 180)
					(length 5.08)
					(name "Q9"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "13"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -2.54 180)
					(length 5.08)
					(name "Q10"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "15"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -7.62 180)
					(length 5.08)
					(name "Q12"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -10.16 180)
					(length 5.08)
					(name "Q13"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 12.7 -12.7 180)
					(length 5.08)
					(name "Q14"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(symbol "4060_1_1"
				(rectangle
					(start -7.62 15.24)
					(end 7.62 -15.24)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
			)
			(embedded_fonts no)
		)
	)
	(rectangle
		(start 83.185 161.29)
		(end 90.805 176.53)
		(stroke
			(width 0)
			(type dot)
			(color 255 0 0 1)
		)
		(fill
			(type none)
		)
		(uuid 1d95e40b-2bfb-46ac-aef7-d61406185c71)
	)
	(rectangle
		(start 55.88 30.48)
		(end 248.92 149.86)
		(stroke
			(width 1)
			(type default)
			(color 200 200 200 1)
		)
		(fill
			(type none)
		)
		(uuid bb86d4de-8a6c-49fd-bb3c-0c8f9cc72e55)
	)
	(text "J. Pieper ADC investigation"
		(exclude_from_sim no)
		(at 142.24 170.18 0)
		(effects
			(font
				(face "Arial")
				(size 1.27 1.27)
				(color 0 0 0 1)
			)
			(justify left bottom)
			(href "https://jpieper.com/2023/07/24/stm32g4-adc-performance-part-2/")
		)
		(uuid "9b3ecc35-3df2-428b-a29e-c6c2c744422e")
	)
	(text "STM32G474 Datasheet p.81"
		(exclude_from_sim no)
		(at 142.24 166.37 0)
		(effects
			(font
				(face "Arial")
				(size 1.27 1.27)
				(color 0 0 0 1)
			)
			(justify left bottom)
			(href "https://www.st.com/resource/en/datasheet/stm32g474cb.pdf")
		)
		(uuid "e6fea1fe-2cf8-4a39-929e-14f4aedafb02")
	)
	(text "AN5346"
		(exclude_from_sim no)
		(at 142.24 162.56 0)
		(effects
			(font
				(face "Arial")
				(size 1.27 1.27)
				(color 0 0 0 1)
			)
			(justify left bottom)
			(href "https://www.st.com/resource/en/application_note/an5346-stm32g4-adc-use-tips-and-recommendations-stmicroelectronics.pdf")
		)
		(uuid "f25578fd-4ab6-4599-95bc-eaa8a509f479")
	)
	(text_box "LAYOUT NOTE:\nblablabla"
		(exclude_from_sim no)
		(at 19.685 148.59 0)
		(size 26.67 11.43)
		(margins 1.4525 1.4525 1.4525 1.4525)
		(stroke
			(width 1)
			(type solid)
			(color 0 0 255 1)
		)
		(fill
			(type none)
		)
		(effects
			(font
				(face "Arial")
				(size 1.27 1.27)
				(thickness 0.4)
				(bold yes)
				(color 0 0 255 1)
			)
			(justify left top)
		)
		(uuid "59800026-abce-490f-af73-e553b627145c")
	)
	(text_box "[${#}] ${TITLE}"
		(exclude_from_sim no)
		(at 115.57 15.24 0)
		(size 72.39 12.7)
		(margins 4.4999 4.4999 4.4999 4.4999)
		(stroke
			(width -0.0001)
			(type default)
		)
		(fill
			(type none)
		)
		(effects
			(font
				(face "Times New Roman")
				(size 6 6)
				(thickness 1.2)
				(bold yes)
				(color 162 22 34 1)
			)
		)
		(uuid "b2c13488-4f2f-433b-bdc6-d210d1646aca")
	)
	(text_box "Block Description"
		(exclude_from_sim no)
		(at 57.15 139.7 0)
		(size 190.5 7.62)
		(margins 1.9049 1.9049 1.9049 1.9049)
		(stroke
			(width -0.0001)
			(type default)
		)
		(fill
			(type none)
		)
		(effects
			(font
				(face "Times New Roman")
				(size 2.54 2.54)
				(thickness 0.508)
				(bold yes)
				(color 162 22 34 1)
			)
			(justify bottom)
		)
		(uuid "b610ad11-6470-4e17-bb6a-df05c5ad2515")
	)
	(text_box "DESIGN NOTE:\nblablabla"
		(exclude_from_sim no)
		(at 48.895 175.26 0)
		(size 21.59 11.43)
		(margins 1.3525 1.3525 1.3525 1.3525)
		(stroke
			(width 0.8)
			(type solid)
			(color 250 236 0 1)
		)
		(fill
			(type none)
		)
		(effects
			(font
				(face "Arial")
				(size 1.27 1.27)
				(color 0 0 0 1)
			)
			(justify left top)
		)
		(uuid "e0003229-9448-4893-9fb1-bea9e839bb75")
	)
	(polyline
		(pts
			(xy 83.185 171.45) (xy 70.485 175.26)
		)
		(stroke
			(width 0)
			(type dot)
			(color 255 0 0 1)
		)
		(uuid "dbc0dbb3-ec35-483a-84d2-c330277e1998")
	)
	(symbol
		(lib_id "4xxx:4020")
		(at 148.59 69.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "48110268-f09a-460b-98ce-8d80141bae2f")
		(property "Reference" "U1"
			(at 150.7333 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "4020"
			(at 150.7333 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" ""
			(at 148.59 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4020bms-24bms-40bms.pdf"
			(at 148.59 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Binary counter 14 stages (asynchronous)"
			(at 148.59 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "2e7eeb68-c2fe-4e78-a8c6-4c8d24dec86d")
		)
		(pin "3"
			(uuid "9a411f1e-3bea-41e8-81aa-2a4f9c2a622f")
		)
		(pin "1"
			(uuid "320dc4a4-59ff-4047-a6f6-5b84823bd042")
		)
		(pin "15"
			(uuid "06843483-8a32-41ae-8f50-b82cc92bc641")
		)
		(pin "16"
			(uuid "be2d6e2f-d501-44c7-a256-bcbb8d2bc67a")
		)
		(pin "11"
			(uuid "f60afc11-7d60-477a-a3fe-af68f069569c")
		)
		(pin "12"
			(uuid "815d96f0-87e1-42c2-a2e0-a303c58a2169")
		)
		(pin "4"
			(uuid "6ad174cd-8a40-42d1-b593-8079a87b0cab")
		)
		(pin "9"
			(uuid "bdc04981-38dd-4c56-9d85-2c603bcb2a9c")
		)
		(pin "8"
			(uuid "f2953b10-b256-4b52-bff3-def08ee6892d")
		)
		(pin "13"
			(uuid "d5a18647-e6ac-44e5-8641-b1fb540f519b")
		)
		(pin "14"
			(uuid "e5d73ea6-e429-437e-8ace-2347dee34ffc")
		)
		(pin "5"
			(uuid "7f4a45c3-3b90-4f79-beb0-de8d84820b8c")
		)
		(pin "6"
			(uuid "883f2fe5-8159-4cd9-9938-d68cf66d2b14")
		)
		(pin "7"
			(uuid "2383c261-3ea9-40d5-848e-1af7dc814074")
		)
		(pin "10"
			(uuid "b7e7f60c-0ee7-41fb-b704-041840702cdd")
		)
		(instances
			(project ""
				(path "/f9e05184-c88b-4a88-ae9c-ab2bdb32be7c/c5103ceb-5325-4a84-a025-9638a412984e/f06537ee-772d-44d3-8c50-e0ba41038c9c"
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "4xxx:4060")
		(at 104.14 72.39 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "ad915d92-65e5-4de4-b04e-3a55aecd6da3")
		(property "Reference" "U2"
			(at 106.2833 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "4060"
			(at 106.2833 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" ""
			(at 104.14 74.93 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/m74hc4060.pdf"
			(at 104.14 77.47 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Binary counter (14-stages) and oscillator"
			(at 104.14 72.39 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "3"
			(uuid "a77a74f7-66ed-45c1-a132-5b5282dfaf5c")
		)
		(pin "9"
			(uuid "9fc88cb6-add6-4ba9-be31-287367f56dd1")
		)
		(pin "13"
			(uuid "c515f573-03be-4234-a277-1fd783aba0a4")
		)
		(pin "14"
			(uuid "0257ebef-d5b7-40ee-8a0b-5e4339a61c0d")
		)
		(pin "6"
			(uuid "1f9fe3d5-818c-4103-91a4-eb8cbeae2c0f")
		)
		(pin "4"
			(uuid "02e45ffd-de78-4730-b925-6ee5fdd8d26f")
		)
		(pin "2"
			(uuid "c38082be-fd84-4719-b154-c7314a5f1ca0")
		)
		(pin "1"
			(uuid "7f65a129-6ca1-48d6-9373-817bfffa5f62")
		)
		(pin "15"
			(uuid "8111adf7-eecc-41c5-8e91-0ca3849a4a04")
		)
		(pin "5"
			(uuid "3c93957f-5363-41c8-b1eb-89c4d39e1fdd")
		)
		(pin "7"
			(uuid "98759940-6efa-4aaf-9879-dcffb1a7b5f0")
		)
		(pin "8"
			(uuid "4b28ed3c-d006-4343-af69-eb82a85d71f3")
		)
		(pin "16"
			(uuid "84d3529e-a171-4d06-bb3d-5beff26ca62b")
		)
		(pin "12"
			(uuid "ca03d2ec-b69e-4999-913a-61960a169264")
		)
		(pin "11"
			(uuid "75ab3c0d-3d74-4d60-9daa-0e95a658322c")
		)
		(pin "10"
			(uuid "729cb0d2-061f-4b28-bcba-15516c3c7bb5")
		)
		(instances
			(project "Nixie_Tube_Clock"
				(path "/f9e05184-c88b-4a88-ae9c-ab2bdb32be7c/c5103ceb-5325-4a84-a025-9638a412984e/f06537ee-772d-44d3-8c50-e0ba41038c9c"
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
)
