{
  "board": {
    "3dviewports": [],
    "design_settings": {
      "defaults": {
        "apply_defaults_to_fp_fields": false,
        "apply_defaults_to_fp_shapes": false,
        "apply_defaults_to_fp_text": false,
        "board_outline_line_width": 0.1,
        "copper_line_width": 0.2,
        "copper_text_italic": false,
        "copper_text_size_h": 1.5,
        "copper_text_size_v": 1.5,
        "copper_text_thickness": 0.3,
        "copper_text_upright": false,
        "courtyard_line_width": 0.05,
        "dimension_precision": 4,
        "dimension_units": 3,
        "dimensions": {
          "arrow_length": 1270000,
          "extension_offset": 500000,
          "keep_text_aligned": true,
          "suppress_zeroes": false,
          "text_position": 0,
          "units_format": 1
        },
        "fab_line_width": 0.1,
        "fab_text_italic": false,
        "fab_text_size_h": 1.0,
        "fab_text_size_v": 1.0,
        "fab_text_thickness": 0.15,
        "fab_text_upright": false,
        "other_line_width": 0.15,
        "other_text_italic": false,
        "other_text_size_h": 1.0,
        "other_text_size_v": 1.0,
        "other_text_thickness": 0.15,
        "other_text_upright": false,
        "pads": {
          "drill": 0.6,
          "height": 1.7,
          "width": 1.7
        },
        "silk_line_width": 0.15,
        "silk_text_italic": false,
        "silk_text_size_h": 1.0,
        "silk_text_size_v": 1.0,
        "silk_text_thickness": 0.15,
        "silk_text_upright": false,
        "zones": {
          "min_clearance": 0.0
        }
      },
      "diff_pair_dimensions": [
        {
          "gap": 0.0,
          "via_gap": 0.0,
          "width": 0.0
        }
      ],
      "drc_exclusions": [],
      "meta": {
        "version": 2
      },
      "rule_severities": {
        "annular_width": "error",
        "clearance": "error",
        "connection_width": "warning",
        "copper_edge_clearance": "error",
        "copper_sliver": "warning",
        "courtyards_overlap": "error",
        "creepage": "error",
        "diff_pair_gap_out_of_range": "error",
        "diff_pair_uncoupled_length_too_long": "error",
        "drill_out_of_range": "error",
        "duplicate_footprints": "warning",
        "extra_footprint": "warning",
        "footprint": "error",
        "footprint_filters_mismatch": "ignore",
        "footprint_symbol_mismatch": "warning",
        "footprint_type_mismatch": "ignore",
        "hole_clearance": "error",
        "hole_near_hole": "error",
        "hole_to_hole": "error",
        "holes_co_located": "warning",
        "invalid_outline": "error",
        "isolated_copper": "warning",
        "item_on_disabled_layer": "error",
        "items_not_allowed": "error",
        "length_out_of_range": "error",
        "lib_footprint_issues": "ignore",
        "lib_footprint_mismatch": "warning",
        "malformed_courtyard": "error",
        "microvia_drill_out_of_range": "error",
        "mirrored_text_on_front_layer": "warning",
        "missing_courtyard": "ignore",
        "missing_footprint": "warning",
        "net_conflict": "warning",
        "nonmirrored_text_on_back_layer": "warning",
        "npth_inside_courtyard": "ignore",
        "padstack": "warning",
        "pth_inside_courtyard": "ignore",
        "shorting_items": "error",
        "silk_edge_clearance": "warning",
        "silk_over_copper": "warning",
        "silk_overlap": "ignore",
        "skew_out_of_range": "error",
        "solder_mask_bridge": "warning",
        "starved_thermal": "error",
        "text_height": "ignore",
        "text_on_edge_cuts": "error",
        "text_thickness": "ignore",
        "through_hole_pad_without_hole": "error",
        "too_many_vias": "error",
        "track_angle": "error",
        "track_dangling": "warning",
        "track_segment_length": "error",
        "track_width": "error",
        "tracks_crossing": "error",
        "unconnected_items": "error",
        "unresolved_variable": "error",
        "via_dangling": "warning",
        "zones_intersect": "error"
      },
      "rules": {
        "max_error": 0.005,
        "min_clearance": 0.2,
        "min_connection": 0.0,
        "min_copper_edge_clearance": 0.25,
        "min_groove_width": 0.0,
        "min_hole_clearance": 0.254,
        "min_hole_to_hole": 0.254,
        "min_microvia_diameter": 0.2,
        "min_microvia_drill": 0.1,
        "min_resolved_spokes": 1,
        "min_silk_clearance": 0.0,
        "min_text_height": 0.8,
        "min_text_thickness": 0.15,
        "min_through_hole_diameter": 0.25,
        "min_track_width": 0.2,
        "min_via_annular_width": 0.15,
        "min_via_diameter": 0.55,
        "solder_mask_clearance": 0.0,
        "solder_mask_min_width": 0.0,
        "solder_mask_to_copper_clearance": 0.0,
        "use_height_for_length_calcs": true
      },
      "teardrop_options": [
        {
          "td_onpthpad": true,
          "td_onroundshapesonly": false,
          "td_onsmdpad": true,
          "td_ontrackend": false,
          "td_onvia": true
        }
      ],
      "teardrop_parameters": [
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 1,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_round_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 1,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_rect_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 1,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_track_end",
          "td_width_to_size_filter_ratio": 0.9
        }
      ],
      "track_widths": [
        0.0,
        0.15,
        0.2,
        0.25,
        0.3,
        0.35,
        0.4,
        0.5
      ],
      "tuning_pattern_settings": {
        "diff_pair_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 1.0
        },
        "diff_pair_skew_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        },
        "single_track_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        }
      },
      "via_dimensions": [
        {
          "diameter": 0.0,
          "drill": 0.0
        },
        {
          "diameter": 0.55,
          "drill": 0.25
        },
        {
          "diameter": 0.6,
          "drill": 0.3
        },
        {
          "diameter": 0.7,
          "drill": 0.3
        },
        {
          "diameter": 0.8,
          "drill": 0.4
        }
      ],
      "zones_allow_external_fillets": false
    },
    "ipc2581": {
      "dist": "",
      "distpn": "",
      "internal_id": "",
      "mfg": "",
      "mpn": ""
    },
    "layer_pairs": [],
    "layer_presets": [],
    "viewports": []
  },
  "boards": [],
  "cvpcb": {
    "equivalence_files": []
  },
  "erc": {
    "erc_exclusions": [],
    "meta": {
      "version": 0
    },
    "pin_map": [
      [
        0,
        0,
        0,
        0,
        0,
        0,
        1,
        0,
        0,
        0,
        0,
        2
      ],
      [
        0,
        2,
        0,
        1,
        0,
        0,
        1,
        0,
        2,
        2,
        2,
        2
      ],
      [
        0,
        0,
        0,
        0,
        0,
        0,
        1,
        0,
        1,
        0,
        1,
        2
      ],
      [
        0,
        1,
        0,
        0,
        0,
        0,
        1,
        1,
        2,
        1,
        1,
        2
      ],
      [
        0,
        0,
        0,
        0,
        0,
        0,
        1,
        0,
        0,
        0,
        0,
        2
      ],
      [
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        0,
        2
      ],
      [
        1,
        1,
        1,
        1,
        1,
        0,
        1,
        1,
        1,
        1,
        1,
        2
      ],
      [
        0,
        0,
        0,
        1,
        0,
        0,
        1,
        0,
        0,
        0,
        0,
        2
      ],
      [
        0,
        2,
        1,
        2,
        0,
        0,
        1,
        0,
        2,
        2,
        2,
        2
      ],
      [
        0,
        2,
        0,
        1,
        0,
        0,
        1,
        0,
        2,
        0,
        0,
        2
      ],
      [
        0,
        2,
        1,
        1,
        0,
        0,
        1,
        0,
        2,
        0,
        0,
        2
      ],
      [
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2,
        2
      ]
    ],
    "rule_severities": {
      "bus_definition_conflict": "error",
      "bus_entry_needed": "error",
      "bus_to_bus_conflict": "error",
      "bus_to_net_conflict": "error",
      "conflicting_netclasses": "error",
      "different_unit_footprint": "error",
      "different_unit_net": "error",
      "duplicate_reference": "error",
      "duplicate_sheet_names": "error",
      "endpoint_off_grid": "warning",
      "extra_units": "error",
      "footprint_filter": "ignore",
      "footprint_link_issues": "warning",
      "four_way_junction": "ignore",
      "global_label_dangling": "warning",
      "hier_label_mismatch": "error",
      "label_dangling": "error",
      "label_multiple_wires": "warning",
      "lib_symbol_issues": "warning",
      "lib_symbol_mismatch": "warning",
      "missing_bidi_pin": "warning",
      "missing_input_pin": "warning",
      "missing_power_pin": "error",
      "missing_unit": "warning",
      "multiple_net_names": "warning",
      "net_not_bus_member": "warning",
      "no_connect_connected": "warning",
      "no_connect_dangling": "warning",
      "pin_not_connected": "error",
      "pin_not_driven": "error",
      "pin_to_pin": "error",
      "power_pin_not_driven": "error",
      "same_local_global_label": "warning",
      "similar_label_and_power": "warning",
      "similar_labels": "warning",
      "similar_power": "warning",
      "simulation_model_issue": "ignore",
      "single_global_label": "ignore",
      "unannotated": "error",
      "unconnected_wire_endpoint": "warning",
      "undefined_netclass": "error",
      "unit_value_mismatch": "error",
      "unresolved_variable": "error",
      "wire_dangling": "error"
    }
  },
  "libraries": {
    "pinned_footprint_libs": [],
    "pinned_symbol_libs": []
  },
  "meta": {
    "filename": "Nixie_Tube_Clock.kicad_pro",
    "version": 3
  },
  "net_settings": {
    "classes": [
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Default",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 2147483647,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "via_diameter": 0.55,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.28,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2032,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "CAN Bus",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 0,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "via_diameter": 0.55,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Chassis",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 1,
        "schematic_color": "rgb(139, 103, 213)",
        "track_width": 0.2,
        "via_diameter": 0.55,
        "via_drill": 0.25,
        "wire_width": 24
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "GND",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 2,
        "schematic_color": "rgb(0, 0, 0)",
        "track_width": 0.2,
        "via_diameter": 0.55,
        "via_drill": 0.25,
        "wire_width": 24
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "High Power",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 3,
        "schematic_color": "rgb(177, 11, 198)",
        "track_width": 0.2,
        "via_diameter": 0.7,
        "via_drill": 0.3,
        "wire_width": 24
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.2,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Kelvin Diff Pair",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 4,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "via_diameter": 0.55,
        "via_drill": 0.25,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Power 12V",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 5,
        "schematic_color": "rgb(255, 0, 171)",
        "track_width": 0.2,
        "via_diameter": 0.55,
        "via_drill": 0.25,
        "wire_width": 24
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Power 3V3",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 6,
        "schematic_color": "rgb(220, 142, 0)",
        "track_width": 0.2,
        "via_diameter": 0.55,
        "via_drill": 0.25,
        "wire_width": 24
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Power 5V",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 7,
        "schematic_color": "rgb(212, 0, 32)",
        "track_width": 0.2,
        "via_diameter": 0.55,
        "via_drill": 0.25,
        "wire_width": 24
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Power A3V3",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 8,
        "schematic_color": "rgb(162, 155, 0)",
        "track_width": 0.2,
        "via_diameter": 0.55,
        "via_drill": 0.25,
        "wire_width": 24
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.28,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2032,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "RS422 Diff Pair",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 9,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "via_diameter": 0.6,
        "via_drill": 0.25,
        "wire_width": 6
      }
    ],
    "meta": {
      "version": 4
    },
    "net_colors": null,
    "netclass_assignments": null,
    "netclass_patterns": [
      {
        "netclass": "RS422 Diff Pair",
        "pattern": "/Project Architecture/Interface - Interconnects/RS422_R+"
      },
      {
        "netclass": "RS422 Diff Pair",
        "pattern": "/Project Architecture/Interface - Interconnects/RS422_R-"
      },
      {
        "netclass": "RS422 Diff Pair",
        "pattern": "/Project Architecture/Interface - Interconnects/RS422_D-"
      },
      {
        "netclass": "RS422 Diff Pair",
        "pattern": "/Project Architecture/Interface - Interconnects/RS422_D+"
      },
      {
        "netclass": "Chassis",
        "pattern": "CHASSIS"
      },
      {
        "netclass": "CAN Bus",
        "pattern": "/Project Architecture/Interface - FD-CAN/FDCAN_P"
      },
      {
        "netclass": "CAN Bus",
        "pattern": "/Project Architecture/Interface - FD-CAN/FDCAN_N"
      },
      {
        "netclass": "Kelvin Diff Pair",
        "pattern": "/Project Architecture/Motor Control - Top Level/SA_P"
      },
      {
        "netclass": "Kelvin Diff Pair",
        "pattern": "/Project Architecture/Motor Control - Top Level/SA_N"
      },
      {
        "netclass": "Kelvin Diff Pair",
        "pattern": "/Project Architecture/Motor Control - Top Level/SB_P"
      },
      {
        "netclass": "Kelvin Diff Pair",
        "pattern": "/Project Architecture/Motor Control - Top Level/SB_N"
      },
      {
        "netclass": "Kelvin Diff Pair",
        "pattern": "/Project Architecture/Motor Control - Top Level/SC_P"
      },
      {
        "netclass": "Kelvin Diff Pair",
        "pattern": "/Project Architecture/Motor Control - Top Level/SC_N"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Motor Control - Top Level/Motor Control - Inverter/PHA"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Motor Control - Top Level/Motor Control - Inverter/PHB"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Motor Control - Top Level/Motor Control - Inverter/PHC"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Motor Control - Top Level/Motor Control - Inverter/SRC_LS_C"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Motor Control - Top Level/Motor Control - Inverter/SRC_LS_B"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Motor Control - Top Level/Motor Control - Inverter/SRC_LS_A"
      },
      {
        "netclass": "High Power",
        "pattern": "+VBAT"
      },
      {
        "netclass": "GND",
        "pattern": "GND"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Power - Generation/VIN_5V"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Power - Generation/VIN_12V"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Power - Generation/F_VBAT_12V"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Power - Generation/F_VBAT_5V"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Power - Generation/F_VIN_5V"
      },
      {
        "netclass": "High Power",
        "pattern": "/Project Architecture/Power - Generation/F_VIN_12V"
      },
      {
        "netclass": "Power 12V",
        "pattern": "+12V"
      },
      {
        "netclass": "Power 12V",
        "pattern": "/Project Architecture/Power - Generation/SW_12V"
      },
      {
        "netclass": "Power 3V3",
        "pattern": "+3V3"
      },
      {
        "netclass": "Power 3V3",
        "pattern": "/Project Architecture/Power - Generation/SW_3V3"
      },
      {
        "netclass": "Power 5V",
        "pattern": "+5V"
      },
      {
        "netclass": "Power 5V",
        "pattern": "/Project Architecture/Power - Generation/SW_5V"
      },
      {
        "netclass": "Power A3V3",
        "pattern": "+A3V3"
      },
      {
        "netclass": "Power A3V3",
        "pattern": "/Project Architecture/MCU - Power/F_A3V3"
      },
      {
        "netclass": "Power 3V3",
        "pattern": "/Project Architecture/Sensing - Position/COMM_VDD"
      },
      {
        "netclass": "Power 3V3",
        "pattern": "/Project Architecture/Sensing - Position/DIS_VDD3V"
      },
      {
        "netclass": "GND",
        "pattern": "/Project Architecture/Interface - Fan Control/FAN_SW"
      },
      {
        "netclass": "Power 5V",
        "pattern": "/Project Architecture/Power - Generation/F_VIN_3V3"
      }
    ]
  },
  "pcbnew": {
    "last_paths": {
      "gencad": "",
      "idf": "",
      "netlist": "KDT_Hierarchical_KiBot.net",
      "plot": "Manufacturing/Fabrication/Gerbers/",
      "pos_files": "",
      "specctra_dsn": "",
      "step": "STEP_Blender/KDT_Hierarchical_KiBot.step",
      "svg": "",
      "vrml": ""
    },
    "page_layout_descr_file": "Templates/KDT_Template_PCB_GIT_A4.kicad_wks"
  },
  "schematic": {
    "annotate_start_num": 0,
    "bom_export_filename": "Manufacturing/Assembly/KDT_Hierarchical_KiBot-bom-k8.csv",
    "bom_fmt_presets": [],
    "bom_fmt_settings": {
      "field_delimiter": ",",
      "keep_line_breaks": false,
      "keep_tabs": false,
      "name": "CSV",
      "ref_delimiter": ",",
      "ref_range_delimiter": "",
      "string_delimiter": "\""
    },
    "bom_presets": [],
    "bom_settings": {
      "exclude_dnp": true,
      "fields_ordered": [
        {
          "group_by": false,
          "label": "#",
          "name": "${ITEM_NUMBER}",
          "show": true
        },
        {
          "group_by": false,
          "label": "Qty",
          "name": "${QUANTITY}",
          "show": true
        },
        {
          "group_by": false,
          "label": "Reference",
          "name": "Reference",
          "show": true
        },
        {
          "group_by": false,
          "label": "Value",
          "name": "Value",
          "show": true
        },
        {
          "group_by": false,
          "label": "Datasheet",
          "name": "Datasheet",
          "show": true
        },
        {
          "group_by": false,
          "label": "Footprint",
          "name": "Footprint",
          "show": true
        },
        {
          "group_by": false,
          "label": "Description",
          "name": "Description",
          "show": true
        },
        {
          "group_by": false,
          "label": "DNP",
          "name": "${DNP}",
          "show": false
        },
        {
          "group_by": false,
          "label": "Manufacturer",
          "name": "Manufacturer",
          "show": true
        },
        {
          "group_by": true,
          "label": "Manufacturer Part Number",
          "name": "Manufacturer Part Number",
          "show": true
        },
        {
          "group_by": false,
          "label": "Config",
          "name": "Config",
          "show": false
        }
      ],
      "filter_string": "",
      "group_symbols": true,
      "include_excluded_from_bom": false,
      "name": "",
      "sort_asc": true,
      "sort_field": "Footprint"
    },
    "connection_grid_size": 50.0,
    "drawing": {
      "dashed_lines_dash_length_ratio": 12.0,
      "dashed_lines_gap_length_ratio": 3.0,
      "default_line_thickness": 6.0,
      "default_text_size": 50.0,
      "field_names": [],
      "intersheets_ref_own_page": false,
      "intersheets_ref_prefix": "",
      "intersheets_ref_short": false,
      "intersheets_ref_show": false,
      "intersheets_ref_suffix": "",
      "junction_size_choice": 3,
      "label_size_ratio": 0.375,
      "operating_point_overlay_i_precision": 3,
      "operating_point_overlay_i_range": "~A",
      "operating_point_overlay_v_precision": 3,
      "operating_point_overlay_v_range": "~V",
      "overbar_offset_ratio": 1.23,
      "pin_symbol_size": 25.0,
      "text_offset_ratio": 0.15
    },
    "legacy_lib_dir": "",
    "legacy_lib_list": [],
    "meta": {
      "version": 1
    },
    "net_format_name": "KiCad",
    "page_layout_descr_file": "kicad-embed://KDT_Template_PCB_A5.kicad_wks",
    "plot_directory": "Schematic/",
    "space_save_all_events": true,
    "spice_current_sheet_as_root": false,
    "spice_external_command": "spice \"%I\"",
    "spice_model_current_sheet_as_root": true,
    "spice_save_all_currents": false,
    "spice_save_all_dissipations": false,
    "spice_save_all_voltages": false,
    "subpart_first_id": 65,
    "subpart_id_separator": 0
  },
  "sheets": [
    [
      "f9e05184-c88b-4a88-ae9c-ab2bdb32be7c",
      "Root"
    ],
    [
      "82da9dbf-ba38-4d08-ba35-a220fa2963b1",
      "Block Diagram"
    ],
    [
      "c5103ceb-5325-4a84-a025-9638a412984e",
      "Project Architecture"
    ],
    [
      "f06537ee-772d-44d3-8c50-e0ba41038c9c",
      "Clock - Oscillator & Divider"
    ],
    [
      "e744f3ce-03a6-44a6-8792-1447ef232b9a",
      "MUX Inputs - Time Logic"
    ],
    [
      "5fb05893-0da3-4f58-a52b-cb6d6f4cb80b",
      "Power - Sequencing"
    ],
    [
      "6e125bd6-2f99-4e5d-b3ea-4899f4540739",
      "Revision History"
    ],
    [
      "2a8f5d5f-cd49-42b0-95eb-45963ec7e9fa",
      "MUX Inputs - Anti-Poisoning Logic"
    ],
    [
      "eafdb10b-8bee-44fc-a926-9f80434f1164",
      "Switching MUX"
    ],
    [
      "b0dd3d99-d7aa-4c74-be83-cbd53dc43e16",
      "MUX Inputs - Date Logic"
    ]
  ],
  "text_variables": {
    "ASSEMBLY_NOTES": "",
    "BOARD_NAME": "Nixie Clock Main Board",
    "COMPANY": "Company Name",
    "DESIGNER": "Aidan Brzezinski",
    "FABRICATION_NOTES": "",
    "GIT_HASH_PCB": "1d094e6",
    "GIT_HASH_SCH": "17a83c7",
    "GIT_URL": "https://git.lokislair.com/aidanbrzezinski/Nixie_Tube_Clock.git",
    "PROJECT_NAME": "Nixie Tube Clock",
    "RELEASE_BODY_1.0.0": "",
    "RELEASE_BODY_1.0.1": "",
    "RELEASE_BODY_1.0.2": "",
    "RELEASE_BODY_1.1.0": "",
    "RELEASE_BODY_UNRELEASED": "Version Unreleased not found.",
    "RELEASE_DATE": "09-Mar-2026",
    "RELEASE_DATE_NUM": "2026-03-09",
    "RELEASE_TITLE_1.0.0": "",
    "RELEASE_TITLE_1.0.1": "",
    "RELEASE_TITLE_1.0.2": "",
    "RELEASE_TITLE_1.1.0": "",
    "RELEASE_TITLE_UNRELEASED": "Version Unreleased not found.",
    "REVISION": "+ (Unreleased)",
    "SHEET_NAME_1": "Cover Page",
    "SHEET_NAME_10": "MUX Inputs - Date Logic",
    "SHEET_NAME_11": "......................................",
    "SHEET_NAME_12": "......................................",
    "SHEET_NAME_13": "......................................",
    "SHEET_NAME_14": "......................................",
    "SHEET_NAME_15": "......................................",
    "SHEET_NAME_16": "......................................",
    "SHEET_NAME_17": "......................................",
    "SHEET_NAME_18": "......................................",
    "SHEET_NAME_19": "......................................",
    "SHEET_NAME_2": "Block Diagram",
    "SHEET_NAME_20": "......................................",
    "SHEET_NAME_21": "......................................",
    "SHEET_NAME_22": "......................................",
    "SHEET_NAME_23": "......................................",
    "SHEET_NAME_24": "......................................",
    "SHEET_NAME_25": "......................................",
    "SHEET_NAME_26": "......................................",
    "SHEET_NAME_27": "......................................",
    "SHEET_NAME_28": "......................................",
    "SHEET_NAME_29": "......................................",
    "SHEET_NAME_3": "Project Architecture",
    "SHEET_NAME_30": "......................................",
    "SHEET_NAME_31": "......................................",
    "SHEET_NAME_32": "......................................",
    "SHEET_NAME_33": "......................................",
    "SHEET_NAME_34": "......................................",
    "SHEET_NAME_35": "......................................",
    "SHEET_NAME_36": "......................................",
    "SHEET_NAME_37": "......................................",
    "SHEET_NAME_38": "......................................",
    "SHEET_NAME_39": "......................................",
    "SHEET_NAME_4": "Clock - Oscillator & Divider",
    "SHEET_NAME_40": "......................................",
    "SHEET_NAME_5": "MUX Inputs - Time Logic",
    "SHEET_NAME_6": "Power - Sequencing",
    "SHEET_NAME_7": "Revision History",
    "SHEET_NAME_8": "MUX Inputs - Anti-Poisoning Logic",
    "SHEET_NAME_9": "Switching MUX",
    "VARIANT": "DRAFT"
  }
}