(fp_lib_table
  (version 7)
  (lib (name "0_package_SO")         (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_package_SO.pretty")          (options "") (descr "SOIC SOP SSOP packages - standard IC packages"))
  (lib (name "0_package_SOT_TO_SMD") (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_package_SOT_TO_SMD.pretty")  (options "") (descr "SOT-23 TO-252 TO-263 SMD transistor and regulator packages"))
  (lib (name "0_package_QFP")        (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_package_QFP.pretty")         (options "") (descr "QFP LQFP quad flat packages"))
  (lib (name "0_package_DFN_QFN")    (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_package_DFN_QFN.pretty")     (options "") (descr "DFN QFN leadless packages"))
  (lib (name "0_package_SON")        (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_package_SON.pretty")         (options "") (descr "SON small outline no-lead packages"))
  (lib (name "0_capacitor_smd")      (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_capacitor_smd.pretty")       (options "") (descr "SMD capacitor footprints - 0201 0402 0603 0805 etc"))
  (lib (name "0_resistor_smd")       (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_resistor_smd.pretty")        (options "") (descr "SMD resistor footprints - 0201 0402 0603 0805 etc"))
  (lib (name "0_inductor_smd")       (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_inductor_smd.pretty")        (options "") (descr "SMD inductor and ferrite bead footprints"))
  (lib (name "0_diode_smd")          (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_diode_smd.pretty")           (options "") (descr "SMD diode footprints - SOD SMA SMB SMC DO-214"))
  (lib (name "0_led_smd")            (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_led_smd.pretty")             (options "") (descr "SMD LED footprints"))
  (lib (name "0_transistor_fet")     (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_transistor_fet.pretty")      (options "") (descr "Transistor and FET footprints - SOT TO through-hole"))
  (lib (name "0_connector")          (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_connector.pretty")           (options "") (descr "All connector footprints - barrel jack JST XT60 pin headers"))
  (lib (name "0_switch_button")      (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_switch_button.pretty")       (options "") (descr "Switch and tactile button footprints"))
  (lib (name "0_switching_regulator")(type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_switching_regulator.pretty") (options "") (descr "Switching regulator and power module footprints"))
  (lib (name "0_interface_uart")     (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_interface_uart.pretty")      (options "") (descr "Interface connector footprints - UART SPI I2C debug headers"))
  (lib (name "0_testpoint")          (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_testpoint.pretty")           (options "") (descr "Test point footprints"))
  (lib (name "0_fiducials")          (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_fiducials.pretty")           (options "") (descr "Fiducial marker footprints for pick and place"))
  (lib (name "0_pad")                (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_pad.pretty")                 (options "") (descr "Bare copper pad footprints - heatsink pads thermal vias"))
  (lib (name "0_net_tie")            (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_net_tie.pretty")             (options "") (descr "Net tie footprints for intentional net connections"))
  (lib (name "0_mousebites")         (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_mousebites.pretty")          (options "") (descr "Mouse bite footprints for PCB panel breakaway tabs"))
  (lib (name "0_custom")             (type "KiCad") (uri "${KIPRJMOD}/lib/shared/footprints/0_custom.pretty")              (options "") (descr "Custom footprints with no standard KiCad equivalent - IN-14 HV5622 NCH6300HV EC11"))
)
